#################################################################
#																#
#	configuration file for ATS Panasonic						#
#																#
#################################################################

# =============== START configuration of line 0 ===============
{CONFIG	line0}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0000
{/CONFIG line0}

{CONFIG	line1}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0101
{/CONFIG line1}
# =============== END configuration of line 0 ===============

{CONFIG	line2}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0202
{/CONFIG line2}


{CONFIG	line3}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0303
{/CONFIG line3}


{CONFIG	line4}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0404
{/CONFIG line4}


{CONFIG	line5}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0505
{/CONFIG line5}

{CONFIG	line6}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0606
{/CONFIG line6}



{CONFIG	line7}
    # ===== physical parameters
	THRESHOLD_ATC_HI	ALL		= 0xa8
	THRESHOLD_TA_HI		ALL		= 0xa8
	THRESHOLD_ATC_LO	ALL		= 0x58
	THRESHOLD_TA_LO		ALL		= 0x58
	DAC_ATC_LO			ALL		= 0
	DAC_TA_LO			ALL		= 0
	DAC_ATC_HI			ALL		= 0xFF
	DAC_TA_HI			ALL		= 0xFF
	ADC_GAIN_ATC		ALL		= 0x00
	ADC_GAIN_TA			ALL		= 0x00

    # ===== packet parameters
	PACKET_LENGTH		ALL		= 24
	DESCREMBLER_TYPE	ALL		= 0
	MASK_B1				ALL		= 0x0001FE00
	MASK_B2				ALL		= 0x000001FE
	REORDER_D			ALL		= 0
	MASK_D				ALL		= 0x00060000
	MASK_PARITY			ALL		= 1
	MASK_1				ALL		= 0x00A80000
	MASK_0				ALL		= 0x00500000
	SCRIPT						= 0x01000000

	CFG_FREQ_PERIOD		= 0x1F
	CFG_DATA_FIXED		= 0x07
	CFG_BIT_ENABLE		= 0x17
	CFG_SELECTOR		= 0x02
	CFG_LB_START_SEQ	= 0x00FF
	CFG_LB_MASK			= 0x0FFF
	CFG_HB_START_SEQ	= 0x00FF
	CFG_HB_MASK			= 0x00FF
	CFG_LH_COUNT		= 0x0043

    # ===== DSP parameters
	DSP_DETECT_TASK		ALL		= 0x0390
	IN_SOUND_FORMAT		ALL		= 0x03
	VAD_LEVEL			ALL		= 0
	AGC_LEVEL			ALL		= 0
	EMUL_SIZE_10MS				= 480
	SET_LINE					= 0x0707
{/CONFIG line7}

# =============== START section commands ===============
{COMMAND}
	line0		MONITOR_ON
	line1		MONITOR_ON
	line2		MONITOR_ON
	line3		MONITOR_ON
	line4		MONITOR_ON
	line5		MONITOR_ON
	line6		MONITOR_ON
	line7		MONITOR_ON
{/COMMAND}
# =============== END section commands ===============